# axis2_transport_receiver.h

Go to the documentation of this file.

    00001 /*
    00002  * Licensed to the Apache Software Foundation (ASF) under one or more
    00003  * contributor license agreements.  See the NOTICE file distributed with
    00004  * this work for additional information regarding copyright ownership.
    00005  * The ASF licenses this file to You under the Apache License, Version 2.0
    00006  * (the "License"); you may not use this file except in compliance with
    00007  * the License.  You may obtain a copy of the License at
    00008  *
    00009  *      http://www.apache.org/licenses/LICENSE-2.0
    00010  *
    00011  * Unless required by applicable law or agreed to in writing, software
    00012  * distributed under the License is distributed on an "AS IS" BASIS,
    00013  * WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
    00014  * See the License for the specific language governing permissions and
    00015  * limitations under the License.
    00016  */
    00017
    00018 #ifndef AXIS2_TRANSPORT_RECEIVER_H
    00019 #define AXIS2_TRANSPORT_RECEIVER_H
    00020
    00039  #include <axis2_const.h>
    00040  #include <axutil_error.h>
    00041  #include <axis2_defines.h>
    00042  #include <axutil_env.h>
    00043  #include <axutil_allocator.h>
    00044  #include <axis2_endpoint_ref.h>
    00045  #include <axis2_ctx.h>
    00046  #include <axis2_conf_ctx.h>
    00047
    00048
    00049 #ifdef __cplusplus
    00050 extern "C"
    00051 {
    00052 #endif
    00053
    00054     struct axis2_conf_ctx;
    00055     struct axis2_transport_in_desc;
    00056
    00058     typedef struct axis2_transport_receiver axis2_transport_receiver_t;
    00059
    00061     typedef struct axis2_transport_receiver_ops axis2_transport_receiver_ops_t;
    00062
    00067     struct axis2_transport_receiver_ops
    00068     {
    00069
    00076         axis2_status_t(AXIS2_CALL * init)(
    00077             axis2_transport_receiver_t * transport_receiver,
    00078             const axutil_env_t * env,
    00079             struct axis2_conf_ctx * conf_ctx,
    00080             struct axis2_transport_in_desc * transport_in);
    00081
    00086         axis2_status_t(AXIS2_CALL * start)(
    00087             axis2_transport_receiver_t * transport_receiver,
    00088             const axutil_env_t * env);
    00089
    00095         axis2_endpoint_ref_t *(AXIS2_CALL * get_reply_to_epr)(
    00096             axis2_transport_receiver_t * transport_receiver,
    00097             const axutil_env_t * env,
    00098             const axis2_char_t * svc_name);
    00099
    00104         struct axis2_conf_ctx *(AXIS2_CALL * get_conf_ctx)(
    00105             axis2_transport_receiver_t * server,
    00106             const axutil_env_t * env);
    00107
    00112         axis2_bool_t(AXIS2_CALL * is_running)(
    00113             axis2_transport_receiver_t * server,
    00114             const axutil_env_t * env);
    00115
    00120         axis2_status_t(AXIS2_CALL * stop)(
    00121             axis2_transport_receiver_t * transport_receiver,
    00122             const axutil_env_t * env);
    00123
    00129         void(AXIS2_CALL * free)(
    00130             axis2_transport_receiver_t * transport_receiver,
    00131             const axutil_env_t * env);
    00132
    00133     };
    00134
    00138     struct axis2_transport_receiver
    00139     {
    00140         const axis2_transport_receiver_ops_t *ops;
    00141     };
    00142
    00145     AXIS2_EXTERN void AXIS2_CALL
    00146     axis2_transport_receiver_free(
    00147         axis2_transport_receiver_t * transport_receiver,
    00148         const axutil_env_t * env);
    00149
    00152     AXIS2_EXTERN axis2_status_t AXIS2_CALL
    00153     axis2_transport_receiver_init(
    00154         axis2_transport_receiver_t * transport_receiver,
    00155         const axutil_env_t * env,
    00156         struct axis2_conf_ctx *conf_ctx,
    00157         struct axis2_transport_in_desc *transport_in);
    00158
    00161     AXIS2_EXTERN axis2_status_t AXIS2_CALL
    00162     axis2_transport_receiver_start(
    00163         axis2_transport_receiver_t * transport_receiver,
    00164         const axutil_env_t * env);
    00165
    00168     AXIS2_EXTERN axis2_status_t AXIS2_CALL
    00169     axis2_transport_receiver_stop(
    00170         axis2_transport_receiver_t * transport_receiver,
    00171         const axutil_env_t * env);
    00172
    00175     AXIS2_EXTERN axis2_endpoint_ref_t *AXIS2_CALL
    00176     axis2_transport_receiver_get_reply_to_epr(
    00177         axis2_transport_receiver_t * transport_receiver,
    00178         const axutil_env_t * env,
    00179         const axis2_char_t * svc_name);
    00180
    00183     AXIS2_EXTERN struct axis2_conf_ctx *AXIS2_CALL
    00184     axis2_transport_receiver_get_conf_ctx(
    00185         axis2_transport_receiver_t * transport_receiver,
    00186         const axutil_env_t * env);
    00187
    00190     AXIS2_EXTERN axis2_bool_t AXIS2_CALL
    00191     axis2_transport_receiver_is_running(
    00192         axis2_transport_receiver_t * transport_receiver,
    00193         const axutil_env_t * env);
    00194
    00197 #ifdef __cplusplus
    00198 }
    00199 #endif
    00200 #endif                          /* AXIS2_TRANSPORT_RECEIVER_H */